{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","39","40"]
["","","Mesatar","dBA","34","34"]
["","","Funksionim pa zhurmë","dBA","21","21"]
["","","I ulët","dBA","28","28"]
["","Ftohje","Mesatar","dBA","33","33"]
["","","Funksionim pa zhurmë","dBA","20","20"]
["","","I ulët","dBA","25","26"]
["","","I lartë","dBA","39","40"]
["Aksesore Standarde","Manual instalimi","","","1","1"]
["","Manual përdorimi","","","1","1"]
["","Telekomandë me rreze infra të kuqe","","","1","1"]
["","Bateri AAA me qeliza të thata","","","2","2"]
["","Mbajtës telekomande","","","1","1"]
["","Pllakë montimi","","","1","1"]
["","Vida mbërthimi për njësinë e brendshme","","","2","2"]
["Sistemet e kontrollit","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Telekomandë me rreze infra të kuqe","","","ARC470A1","ARC470A1"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35","6.35"]
["","Gazi","Dia. jasht.","mm","9.50","9.50"]
["","Drain","","","18","18"]
["Fuqia në hyrje","Ftohje","Nom.","kW","0.017","0.019"]
["","Ngrohje","Nom.","kW","0.020","0.020"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","55","55"]
["","Ngrohje","","dBA","55","55"]
["Dimensionet","Njësia","Gjerësia","mm","770","770"]
["","","Thellësia","mm","225","225"]
["","","Lartësia","mm","286","286"]
["Veshja e jashtme","Colour","","","E bardhë","E bardhë"]
["Pesha","Njësia","","kg","8.50","8.50"]
["Power supply","Faza","","","1~","1~"]
["","Frekuenca","","Hz","50","50"]
["","Tensioni","","V","220-240","220-240"]