{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":11,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F"]
[]
[]
[]
[]
["","","","","","FTXF20F5V1B","FTXF25F5V1B (Archived)","FTXF35F5V1B (Archived)","FTXF42F5V1B (Archived)","FTXF50F5V1B (Archived)","FTXF60F2V1B (Archived)"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.023","0.023","0.029","0.04","0.04","0.032"]
["","Ngrohje","","Nom.","kW","0.023","0.023","0.029","0.04","0.04","0.035"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","286","286","286","286","286","295"]
["","","","Gjerësia","mm","770","770","770","770","770","990"]
["","","","Thellësia","mm","225","225","225","225","225","263"]
["Pesha","Njësia","","","kg","8","8","8.5","9","9","13.5"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","9.8","10","11.5","12.6","12.6","17.3"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","8","8","8","9","9","14.8"]
["","","","I ulët","m³/min","6","6.2","6.4","6.9","7.2","12.2"]
["","","","Funksionim pa zhurmë","m³/min","4.3","4.3","4.4","4.9","6.4","10.7"]
["","","Ngrohje","I lartë","m³/min","10.4","10.4","11.9","12.8","12.8","17.9"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","8.3","8.4","8.6","8.8","9.6","15.8"]
["","","Ngrohje","I ulët","m³/min","6.2","6.4","6.5","6.7","7.2","12.8"]
["","","","Funksionim pa zhurmë","m³/min","5.3","5.3","5.3","5.2","6.4","11.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","53","54","54","59","59","60"]
["","Ngrohje","","","dBA","55","55","56","59","59","62"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","39","40","43","45","45","45"]
["","","","Mesatar","dBA","33","33","34","36","39","41"]
["","","","I ulët","dBA","25","26","27","30","34","36"]
["","","","Funksionim pa zhurmë","dBA","20","20","20","22","31","33"]
["","Ngrohje","","I lartë","dBA","39","40","40","44","44","44"]
["","","","Mesatar","dBA","34","34","35","34","38","40"]
["","","","I ulët","dBA","28","28","29","28","33","35"]
["","","","Funksionim pa zhurmë","dBA","21","21","21","22","30","32"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6","6","6","6","6","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","9.5","9.5","9.5","12.7","12.7"]
["","Kullimi","","","","18","18","18","18","18","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC480A93","ARC470A1"]
["","Telekomandë me tela","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Aksesore Standarde","Installation manual","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["Furnizimi me energji","Emri","","","","","","","","","V1"]
["","Faza","","","","1~","1~","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50","50","50"]
["","Tensioni","","","V","220-440","220-440","220-440","220-440","220-440","220-240"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)"]
["","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]