{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AS"]
[]
[]
[]
[]
["","","","","","FTXJ20A2V1BS","FTXJ25A2V1BS","FTXJ35A2V1BS","FTXJ42A2V1BS","FTXJ50A2V1BS"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.02","0.022","0.024","0.028","0.031"]
["","Ngrohje","","Nom.","kW","0.021","0.022","0.024","0.036","0.039"]
["Veshja e jashtme","Ngjyra","","","","Argjend","Argjend","Argjend","Argjend","Argjend"]
["Dimensionet","Njësia","","Lartësia","mm","305","305","305","305","305"]
["","","","Gjerësia","mm","900","900","900","900","900"]
["","","","Thellësia","mm","212","212","212","212","212"]
["Pesha","Njësia","","","kg","12","12","12","12","12"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","11","11.4","11.8","13","13.5"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","8.4","8.6","8.6","9.5","10.4"]
["","","","I ulët","m³/min","6","6","6","7.2","7.6"]
["","","","Funksionim pa zhurmë","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Ngrohje","I lartë","m³/min","11.1","11.3","11.7","14.4","15.0"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","8.7","9","9","10.5","11.1"]
["","","Ngrohje","I ulët","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Funksionim pa zhurmë","m³/min","4.6","4.6","4.6","5.2","5.7"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","57","57","60","60","60"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","39","40","41","45","46"]
["","","","Mesatar","dBA","32","33","33","37","39"]
["","","","I ulët","dBA","25","25","25","29","31"]
["","","","Funksionim pa zhurmë","dBA","19","19","19","21","24"]
["","Ngrohje","","I lartë","dBA","39","40","41","45","46"]
["","","","Mesatar","dBA","32","33","33","37","42"]
["","","","I ulët","dBA","25","25","25","29","33"]
["","","","Funksionim pa zhurmë","dBA","19","19","19","21","24"]
["Agjenti ftohës","GWP","","","","675","675","675","675","675"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","9.5","9.5","12.7","12.7"]
["","Kullimi","","","","18","18","18","18","18"]
["Sistemet e kontrollit","Infrared remote control","","","","ARC488A1S","ARC488A1S","ARC488A1S","ARC488A1S","ARC488A1S"]
["Sistemet e kontrollit","Telekomandë me tela","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Aksesore Standarde","Installation manual","","","","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Furnizimi me energji","Emri","","","","V1","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240","220-240","220-240"]