{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":10,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Kapaciteti ftohës","Nom.","","kW","4.00","","4.00","5.20","4.00","6.00"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","467","","471","593","457","787"]
["","EER","","","4.28","","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","","4.05","4.42","4.04","3.88"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","","A","A","A","A"]
["","","Ngrohje","","A","","A","A","A","A"]
["Kapaciteti ngrohës","Nom.","","kW","4.60","","6.80","6.80","6.50","7.80"]
["Kapaciteti ftohës","Nom.","","kW","","4.00"]
["Kapaciteti ngrohës","Nom.","","kW","","4.60"]
["Efikasiteti nominal","EER","","","","4.15"]
["","COP","","","","3.95"]
["","Konsumi vjetor i energjisë","","kWh","","482"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","A"]
["","","Ngrohje","","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","","A++"]
["","Kapaciteti","Pdesign","kW","","4.00"]
["","SEER","","","","7.62"]
["","Konsumi vjetor i energjisë","","kWh/a","","164"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","","A+"]
["","Kapaciteti","Pdesign","kW","","4.80"]
["","SCOP/A","","","","4.11"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","","3.58"]
["","Konsumi vjetor i energjisë","","kWh/a","","1632"]
["Shënime","","","","","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]