{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["","Ngrohje","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","283","283"]
["","","","Gjerësia","mm","770","770"]
["","","","Thellësia","mm","198","198"]
["Pesha","Njësia","","","kg","8.00","8.00"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","9.3","9.3"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","7.7","7.7"]
["","","","I ulët","m³/min","6.1","6.1"]
["","","","Funksionim pa zhurmë","m³/min","4.9","4.9"]
["","","Ngrohje","I lartë","m³/min","10.1","10.1"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","8.4","8.4"]
["","","Ngrohje","I ulët","m³/min","6.7","6.7"]
["","","","Funksionim pa zhurmë","m³/min","5.7","5.7"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","57","57"]
["","Ngrohje","","","dBA","57","57"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","41","41"]
["","","","Mesatar","dBA","34","34"]
["","","","I ulët","dBA","27","27"]
["","","","Funksionim pa zhurmë","dBA","23","23"]
["","Ngrohje","","I lartë","dBA","41","41"]
["","","","Mesatar","dBA","35","35"]
["","","","I ulët","dBA","29","29"]
["","","","Funksionim pa zhurmë","dBA","26","26"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.50","9.50"]
["","Kullimi","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Batteries","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Furnizimi me energji","Emri","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]