{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","47","47"]
["","","Funksionim pa zhurmë","dBA","19","19"]
["","","I ulët","dBA","23","23"]
["","Ftohje","Funksionim pa zhurmë","dBA","21","21"]
["","","I ulët","dBA","33","33"]
["","","I lartë","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Ftohje","Nom.","dBA","39","39"]
["Aksesore Standarde","Manual instalimi","","","1","1"]
["","Manual përdorimi","","","1","1"]
["","Telekomandë me rreze infra të kuqe","","","1","1"]
["","Bateri","","","2","2"]
["","Mbajtës telekomande","","","1","1"]
["","Pllakë montimi","","","1","1"]
["","Filtër fotokatalitik me apatit titani për pastrimin e ajrit","","","2","2"]
["","Vida mbërthimi për njësinë e brendshme","","","2","2"]
["Control systems","Infrared remote control","","","ARC466A9","ARC466A9"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35","6.35"]
["","Gazi","Dia. jasht.","mm","9.5","9.5"]
["","Kullimi","","","18","18"]
["Fuqia në hyrje","Ftohje","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Ngrohje","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","59","59"]
["","Ngrohje","","dBA","62","62"]
["Dimensionet","Njësia","Gjerësia","mm","900","900"]
["","","Thellësia","mm","215","215"]
["","","Lartësia","mm","298","298"]
["Veshja e jashtme","Ngjyra","","","E bardhë","E bardhë"]
["Pesha","Njësia","","kg","12","12"]
["Power supply","Faza","","","1~","1~"]
["","Frekuenca","","Hz","50","50"]
["","Emri","","","V1","V1"]
["","Tensioni","","V","220-240","220-240"]
["Shënime","","","","(1) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur.","(1) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]