{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":7,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXQ-A"]
[]
[]
[]
[]
["","","","","","FTXQ25AMV1B","FTXQ35AMV1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","","42.0"]
["","","","Mesatar","dBA","","35.0"]
["","","","Funksionim pa zhurmë","dBA","","25.0"]
["","","","I ulët","dBA","","30.0"]
["","Ftohje","","Mesatar","dBA","","35.0"]
["","","","Funksionim pa zhurmë","dBA","","24.0"]
["","","","I ulët","dBA","","28.0"]
["","","","I lartë","dBA","","41.0"]
["Aksesore Standarde","Manual instalimi","","","","","1"]
["","Manual përdorimi","","","","","1"]
["","Bateri AAA me qeliza të thata","","","","","2"]
["","Pllakë montimi","","","","","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","","2"]
["","Masat e përgjithshme të sigurisë","","","","","1"]
["","Telekomandë me rreze infra të kuqe","","","","","1"]
["","Mbajtës telekomande","","","","","1"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","ARC470A1"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.50"]
["","Drain","","","","","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.025"]
["","Ngrohje","","Nom.","kW","","0.031"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","55"]
["Dimensionet","Njësia","","Gjerësia","mm","","770"]
["","","","Thellësia","mm","","232"]
["","","","Lartësia","mm","","291"]
["Veshja e jashtme","Colour","","","","","E bardhë"]
["Pesha","Njësia","","","kg","","9.00"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","","12.0"]
["","","","I ulët","m³/min","","8.3"]
["","","","Mesatar","m³/min","","10.0"]
["","","","Funksionim pa zhurmë","m³/min","","6.9"]
["","","Cooling","I ulët","m³/min","","7.0"]
["","","","Mesatar","m³/min","","8.5"]
["","","","I lartë","m³/min","","10.5"]
["","","","Funksionim pa zhurmë","m³/min","","6.0"]
["Power supply","Faza","","","","","1~"]
["","Frekuenca","","","Hz","","50"]
["","Tensioni","","","V","","220-240"]
["Shënime","","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19.0°CWB; temperatura e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m"]
["","","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.023"]
["","Ngrohje","","Nom.","kW","0.027"]
["Veshja e jashtme","Ngjyra","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","291"]
["","","","Gjerësia","mm","770"]
["","","","Thellësia","mm","232"]
["Pesha","Njësia","","","kg","9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","10.2"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","8.1"]
["","","","I ulët","m³/min","6.5"]
["","","","Funksionim pa zhurmë","m³/min","5"]
["","","Ngrohje","I lartë","m³/min","11.1"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","9.6"]
["","","Ngrohje","I ulët","m³/min","8.1"]
["","","","Funksionim pa zhurmë","m³/min","6.8"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","55"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","40"]
["","","","Mesatar","dBA","34"]
["","","","I ulët","dBA","26"]
["","","","Funksionim pa zhurmë","dBA","23"]
["","Ngrohje","","I lartë","dBA","40"]
["","","","Mesatar","dBA","34"]
["","","","I ulët","dBA","29"]
["","","","Funksionim pa zhurmë","dBA","25"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5"]
["","Kullimi","","","","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARC470A1"]
["Aksesore Standarde","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]