{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","38","39","42","42","44","","46"]
["","","","Funksionim pa zhurmë","dBA","25","25","26","30","31","","34"]
["","","","I ulët","dBA","28","28","29","33","34","","37"]
["","Ftohje","","Funksionim pa zhurmë","dBA","22","22","23","30","31","","34"]
["","","","I ulët","dBA","25","25","26","33","34","","37"]
["","","","I lartë","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Ftohje","","Nom.","dBA","32","32","34","38","39","","42"]
["Aksesore Standarde","Filtër fotokatalitik me apatit titani për pastrimin e ajrit","","","","2","2","2","2","2"]
["","Manual përdorimi","","","","1","1","1","1","1","","1"]
["","Manual instalimi","","","","1","1","1","1","1","","1"]
["","Telekomandë me valë","","","","1","1","1","1","1","","1"]
["","Bateri","","","","2","2","2","2","2","","2"]
["","Mbajtës telekomande","","","","1","1","1","1","1","","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2","2","2","2","2","","2"]
["","Pllakë montimi","","","","1","1","1","1","1","","1"]
["Control systems","Infrared remote control","","","","","","","","","","ARC452A3"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gazi","","Dia. jasht.","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Kullimi","","","","18","18","18","18","18","","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Ngrohje","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Ftohje","","","dBA","54","54","58","58","59","","63"]
["","Ngrohje","","","dBA","54","55","58","58","60","","62"]
["Dimensionet","Njësia","","Gjerësia","mm","800","800","800","800","800","","1,050"]
["","","","Thellësia","mm","215","215","215","215","215","","250"]
["","","","Lartësia","mm","295","295","295","295","295","","290"]
["Casing","Colour","","","","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë","","E bardhë"]
["Pesha","Njësia","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frekuenca","","","Hz","50","50","50","50","50","","50"]
["","Emri","","","","V1","V1","V1","V1","V1","","V1"]
["","Tensioni","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","Nom.","m³/min","","","","","","16.0"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","","","","","","41"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Nom.","m³/min","","","","","","14.9"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","","","","","","40"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Ngrohje","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Veshja e jashtme","Ngjyra","","","","","","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","","","","","290"]
["","","","Gjerësia","mm","","","","","","1050"]
["","","","Thellësia","mm","","","","","","250"]
["Pesha","Njësia","","","kg","","","","","","12"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","","","","","16.0"]
["","","","I ulët","m³/min","","","","","","11.3"]
["","","","Funksionim pa zhurmë","m³/min","","","","","","10.1"]
["","","Ngrohje","I lartë","m³/min","","","","","","17.2"]
["","","","I ulët","m³/min","","","","","","12.6"]
["","","","Funksionim pa zhurmë","m³/min","","","","","","11.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","","","","","60"]
["","Ngrohje","","","dBA","","","","","","59"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","","","","","45"]
["","","","I ulët","dBA","","","","","","36"]
["","","","Funksionim pa zhurmë","dBA","","","","","","33"]
["","Ngrohje","","I lartë","dBA","","","","","","44"]
["","","","I ulët","dBA","","","","","","35"]
["","","","Funksionim pa zhurmë","dBA","","","","","","32"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","","","","","6.35"]
["","Gazi","","Dia. jasht.","mm","","","","","","12.7"]
["","Kullimi","","","","","","","","","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","","","","","ARC452A3"]
["Aksesore Standarde","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Furnizimi me energji","Emri","","","","","","","","","V1"]
["","Faza","","","","","","","","","1~"]
["","Frekuenca","","","Hz","","","","","","50"]
["","Tensioni","","","V","","","","","","220-240"]
["Aksesore Standarde","Filtër fotokatalitik me apatit titani për pastrimin e ajrit, pa kornizë","","","","","","","","","","2"]
["Shënime","","","","","","","","","","","(4) - 240V"]