{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","40","","","","","","45"]
["","","","Funksionim pa zhurmë","dBA","19","","","","","","22"]
["","","","I ulët","dBA","27","","","","","","33"]
["","Ftohje","","Funksionim pa zhurmë","dBA","19","","","","","","21"]
["","","","I ulët","dBA","24","","","","","","33"]
["","","","I lartë","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Ftohje","","Nom.","dBA","32","","","","","","39"]
["Aksesore Standarde","Manual instalimi","","","","1","","","","","","1"]
["","Manual përdorimi","","","","1","","","","","","1"]
["","Telekomandë me valë","","","","1","","","","","","1"]
["","Bateri","","","","2","","","","","","2"]
["","Mbajtës telekomande","","","","1","","","","","","1"]
["","Pllakë montimi","","","","1","","","","","","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2","","","","","","2"]
["","Filtër fotokatalitik me apatit titani për pastrimin e ajrit","","","","2","","","","","","2"]
["Sistemet e kontrollit","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","","","","","","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","","","","","","9.5"]
["","Kullimi","","","","18","","","","","","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Ngrohje","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Ftohje","","","dBA","58","","","","","","59"]
["","Ngrohje","","","dBA","58","","","","","","59"]
["Dimensionet","Njësia","","Gjerësia","mm","780","","","","","","900"]
["","","","Thellësia","mm","215","","","","","","215"]
["","","","Lartësia","mm","289","","","","","","298"]
["Veshja e jashtme","Colour","","","","E bardhë","","","","","","E bardhë"]
["Pesha","Njësia","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Frekuenca","","","Hz","50","","","","","","50"]
["","Emri","","","","V1","","","","","","V1"]
["","Tensioni","","","V","220-240","","","","","","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Ngrohje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Veshja e jashtme","Ngjyra","","","","","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë","","E bardhë","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","215","289","215","298","215","","215","298","215"]
["","","","Gjerësia","mm","","780","780","780","900","900","","900","900","900"]
["","","","Thellësia","mm","","289","215","289","215","298","","298","215","298"]
["Pesha","Njësia","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","I ulët","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Funksionim pa zhurmë","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Ngrohje","I lartë","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Ngrohje","I ulët","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Funksionim pa zhurmë","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Ngrohje","","","dBA","","58","58","58","59","59","","59","60","60"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Mesatar","dBA","","32","33","33","","37","","39","","40"]
["","","","I ulët","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Funksionim pa zhurmë","dBA","","19","19","19","19","19","","21","23","23"]
["","Ngrohje","","I lartë","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Mesatar","dBA","","34","34","34","","39","","39","","40"]
["","","","I ulët","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Funksionim pa zhurmë","dBA","","19","19","19","19","19","","22","24","24"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Kullimi","","","","","18","18","18","18","18","","18","18","18"]
["Sistemet e kontrollit","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Aksesore Standarde","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Furnizimi me energji","Emri","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Faza","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frekuenca","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Tensioni","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","","","34","","39","","","","40"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Aksesore Standarde","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Shënime","","","","","","","","","","","(4) - 240V"]