{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.032","0.032"]
["","Ngrohje","","Nom.","kW","0.032","0.032"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","286","286"]
["","","","Gjerësia","mm","770","770"]
["","","","Thellësia","mm","225","225"]
["Pesha","Njësia","","","kg","9","9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","11","11"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","7.9","7.9"]
["","","","I ulët","m³/min","5","5"]
["","","","Funksionim pa zhurmë","m³/min","3.7","3.7"]
["","","Ngrohje","I lartë","m³/min","10.5","10.5"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","9","9"]
["","","Ngrohje","I ulët","m³/min","5.5","5.5"]
["","","","Funksionim pa zhurmë","m³/min","4.4","4.4"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","58","58"]
["","Ngrohje","","","dBA","58","58"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","43","43"]
["","","","Mesatar","dBA","35","35"]
["","","","I ulët","dBA","26","26"]
["","","","Funksionim pa zhurmë","dBA","21","21"]
["","Ngrohje","","I lartë","dBA","43","43"]
["","","","Mesatar","dBA","35","35"]
["","","","I ulët","dBA","26","26"]
["","","","Funksionim pa zhurmë","dBA","21","21"]
["Agjenti ftohës","GWP","","","","675","675"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","9.5"]
["","Kullimi","","","","18","18"]
["Sistemet e kontrollit","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Aksesore Standarde","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Furnizimi me energji","Emri","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m"]
["","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["Aksesore Standarde","FTXTP35A5V1B","","","","","1"]