{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","43"]
["","","","Mesatar","dBA","35"]
["","","","Funksionim pa zhurmë","dBA","21"]
["","","","I ulët","dBA","26"]
["","Ftohje","","Medium","dBA","35"]
["","","","Funksionim pa zhurmë","dBA","21"]
["","","","I ulët","dBA","26"]
["","","","I lartë","dBA","43"]
["Aksesore Standarde","Manual instalimi","","","","1"]
["","Manual përdorimi","","","","1"]
["","Telekomandë me valë","","","","1"]
["","Bateri AAA me qeliza të thata","","","","2"]
["","Mbajtës telekomande","","","","1"]
["","Pllakë montimi","","","","1"]
["","Filtër prej apatiti titani për largimin e aromave","","","","2"]
["","Vida mbërthimi për njësinë e brendshme","","","","2"]
["Sistemet e kontrollit","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Liquid","","Dia. jasht.","mm","6.35"]
["","Gas","","Diametri i jashtëm","mm","9.50"]
["","Kullimi","","","","16 (diametri i brendshëm i zorrës lidhëse)"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.030"]
["","Ngrohje","","Nom.","kW","0.035"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","58"]
["","Ngrohje","","","dBA","58"]
["Dimensions","Njësia","","Gjerësia","mm","770"]
["","","","Thellësia","mm","225"]
["","","","Lartësia","mm","285"]
["Veshja e jashtme","Colour","","","","E bardhë"]
["Pesha","Njësia","","","kg","9.0"]
["Power supply","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Name","","","","V1"]
["","Tensioni","","","V","220-240"]
["Shënime","","","","","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.03"]
["","Ngrohje","","Nom.","kW","","0.035"]
["Veshja e jashtme","Ngjyra","","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","285"]
["","","","Gjerësia","mm","","770"]
["","","","Thellësia","mm","","225"]
["Pesha","Njësia","","","kg","","9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","11.4"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","8.2"]
["","","","I ulët","m³/min","","5.4"]
["","","","Funksionim pa zhurmë","m³/min","","4.3"]
["","","Ngrohje","I lartë","m³/min","","10.8"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","7.8"]
["","","Ngrohje","I ulët","m³/min","","5.8"]
["","","","Funksionim pa zhurmë","m³/min","","4.9"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","58"]
["","Ngrohje","","","dBA","","58"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","43"]
["","","","Mesatar","dBA","","35"]
["","","","I ulët","dBA","","26"]
["","","","Funksionim pa zhurmë","dBA","","21"]
["","Ngrohje","","I lartë","dBA","","43"]
["","","","Mesatar","dBA","","35"]
["","","","I ulët","dBA","","26"]
["","","","Funksionim pa zhurmë","dBA","","21"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.5"]
["","Kullimi","","","","","16 (diametri i brendshëm i zorrës lidhëse)"]
["Sistemet e kontrollit","Infrared remote control","","","","","ARC480A11"]
["Sistemet e kontrollit","Telekomandë me tela","","","","","BRC944B2, BRC073A1"]
["Aksesore Standarde","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Furnizimi me energji","Emri","","","","","V1"]
["","Faza","","","","","1~"]
["","Frekuenca","","","Hz","","50"]
["","Tensioni","","","V","","220-240"]