{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","39","42","44"]
["","","","Funksionim pa zhurmë","dBA","19","19","24"]
["","","","I ulët","dBA","28","29","31"]
["","Ftohje","","Funksionim pa zhurmë","dBA","19","19","23"]
["","","","I ulët","dBA","26","27","30"]
["","","","I lartë","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Ftohje","","Nom.","dBA","33","35","38"]
["Aksesore Standarde","Filtër fotokatalitik për pastrimin dhe aromatizimin e ajrit","","","","1","1","1"]
["","Telekomandë me valë","","","","1","1","1"]
["","Bateritë e thata","","","","2","2","2"]
["","Mbajtës telekomande","","","","1","1","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","3","3","3"]
["","Pllakë montimi","","","","1","1","1"]
["Sistemet e kontrollit","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5","9.5","9.5"]
["Power input","Ftohje","","Nom.","kW","0.030","0.030","0.030"]
["","Ngrohje","","Nom.","kW","0.030","0.030","0.030"]
["Sound power level","Ftohje","","","dBA","54","57","60"]
["","Ngrohje","","","dBA","56","57","59"]
["Dimensionet","Njësia","","Gjerësia","mm","798","798","798"]
["","","","Thellësia","mm","372","372","372"]
["","","","Lartësia","mm","295","295","295"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë","E bardhë"]
["Pesha","Njësia","","","kg","15","15","15"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","11.7","13.3","14.4"]
["","","","I ulët","m³/min","6.7","6.9","7.7"]
["","","","Funksionim pa zhurmë","m³/min","4.8","4.8","5.9"]
["","","Ftohje","I ulët","m³/min","5.3","5.6","6.6"]
["","","","I lartë","m³/min","10.7","12.1","15.0"]
["","","","Funksionim pa zhurmë","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Ftohje","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Faza","","","","1~","1~","1~"]
["","Emri","","","","V1","V1","V1"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Pjesa e përparme e shkëmbyesit të nxehtësisë","(4) - Pjesa e përparme e shkëmbyesit të nxehtësisë","(4) - Pjesa e përparme e shkëmbyesit të nxehtësisë"]
["","","","","","(5) - Pjesa e pasme e shkëmbyesit të nxehtësisë","(5) - Pjesa e pasme e shkëmbyesit të nxehtësisë","(5) - Pjesa e pasme e shkëmbyesit të nxehtësisë"]