{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Kapaciteti ftohës","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Ftohja e hapësirës","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","","","371","371","371","371"]
["","Kapaciteti","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","","","","A++","A++","A++","A++"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","","","","A+","A+","A+","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Efikasiteti nominal","Annual energy consumption","","kWh","","","","","","","","","","835","","835"]
["","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["","COP","","","","","","","","","","","","4.08","","4.08"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","","","","","","","","","A","","A"]
["","","Ngrohje","","","","","","","","","","","A","","A"]
["Kapaciteti ngrohës","Nom.","","kW","","","","","","","","","","7.50","","7.50"]
["Shënime","","","","","","","","","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m.","(1) - Shiko skicën e veçantë për diapazonin e funksionimit","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","","","","","","","","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Shënime","","","","","","","","","","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","","","","","","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]