{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","","","","41","46","47"]
["","","","Mesatar","dBA","","","","38","42","43"]
["","","","I ulët","dBA","","","","35","39","40"]
["","Ftohje","","Mesatar","dBA","","","","38","42","43"]
["","","","I ulët","dBA","","","","35","39","40"]
["","","","I lartë","dBA","","","","41","46","47"]
["Aksesore Standarde","Manual përdorimi","","","","","","","1","1","1"]
["","Manual instalimi","","","","","","","1","1","1"]
["","Zorrë kullimi","","","","","","","1","1","1"]
["","Tub termoizolimi","","","","","","","3","3","3"]
["","Fasheta lidhëse për kabllot","","","","","","","10","10","10"]
["","Fashetë","","","","","","","1","1","1"]
["","Material izolues","","","","","","","4","4","4"]
["","Pllakë fiksimi për rondelën","","","","","","","1","1","1"]
["","Nyjë kullimi","","","","","","","1","1","1"]
["","Pëlhurë e pathurur","","","","","","","1","1","1"]
["","Rondele","","","","","","","8","8","8"]
["","Vidë mbërthimi për zorrën e kullimit","","","","","","","5","5","5"]
["Sistemet e kontrollit","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Kapaciteti ftohës","Total capacity","","Nom.","kW","","","","","","12.1"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","","","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","","","","15.9","15.9","15.9"]
["","Kullimi","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","","","59","64","65"]
["","Ngrohje","","","dBA","","","","59","64"]
["Dimensionet","Njësia","","Gjerësia","mm","","","","950","950","950"]
["","","","Thellësia","mm","","","","950","950","950"]
["","","","Lartësia","mm","","","","198","198","198"]
["Veshja e jashtme","Materiali","","","","","","","Rrëshirë","Rrëshirë","Rrëshirë"]
["","Ngjyra","","","","","","","E bardhë e freskët","E bardhë e freskët","E bardhë e freskët"]
["Pesha","Njësia","","","kg","","","","25.0","26.0","26"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","","","","23.0","31.0","32.5"]
["","","","Mesatar","m³/min","","","","19.5","25.5","26.5"]
["","","","I ulët","m³/min","","","","16.0","20.0","20.5"]
["","","Ftohje","I ulët","m³/min","","","","16.0","20.0","20.5"]
["","","","Mesatar","m³/min","","","","19.5","25.5","26.5"]
["","","","I lartë","m³/min","","","","23.0","31.0","32.5"]
["Lartësia e kullimit","mm","","","","","","","600","600","600"]
["Kapaciteti ngrohës","Total capacity","","Nom.","kW","","","","","","13.5"]
["Veshja e jashtme","Ngjyra","","","","E bardhë e freskët","E bardhë e freskët","E bardhë e freskët"]
["","Materiali","","","","Rrëshirë","Rrëshirë","Rrëshirë"]
["Dimensionet","Njësia","","Lartësia","mm","198","198","198"]
["","","","Gjerësia","mm","950","950","950"]
["","","","Thellësia","mm","950","950","950"]
["Pesha","Njësia","","","kg","25.0","26.0","26.0"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","23.0","31.0","32.5"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","19.5","25.5","26.5"]
["","","","I ulët","m³/min","16.0","20.0","20.5"]
["","","Ngrohje","I lartë","m³/min","23.0","31.0","32.5"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","19.5","25.5","26.5"]
["","","Ngrohje","I ulët","m³/min","16.0","20.0","20.5"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","59","64","65"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","41","46","47"]
["","","","Mesatar","dBA","38","42","43"]
["","","","I ulët","dBA","35","39","40"]
["","Ngrohje","","I lartë","dBA","41","46","47"]
["","","","Mesatar","dBA","38","42","43"]
["","","","I ulët","dBA","35","39","40"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","15.9","15.9","15.9"]
["","Kullimi","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Lartësia e kullimit","mm","","","","600","600","600"]
["Aksesore Standarde","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Kapaciteti ftohës","Kapaciteti total","","Nom.","kW","","","12.10"]
["Kapaciteti i ngrohjes","Kapaciteti total","","Nom.","kW","","","13.5"]