{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FUQ71CVEB / RZQG71L9V1B","FUQ100CVEB / RZQG71L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG100L9V1B","FUQ100CVEB / RZQG100L9V1B","FUQ125CVEB / RZQG125L9V1B","FUQ71CVEB / FUQ71CVEB / RZQG125L9V1B"]
["Kapaciteti ftohës","Nom.","","kW","6.8","","","9.5","12.0"]
["Space cooling","SEER","","","6.42","6.50","5.10","6.11","5.61","5.10"]
["","Konsumi vjetor i energjisë","","kWh/a","371","367","652","545","749","824"]
["","Kapaciteti","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Kategoria e efikasitetit të energjisë","","","A++","A++","B","A++","A+","B"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","7.60","7.60","11.30","11.30","14.13","12.71"]
["","SCOP/A","","","4.20","4.20","3.80","4.50","4.44","3.80"]
["","Kategoria e efikasitetit të energjisë","","","A+","A+","A","A+","A+","A"]
["","Konsumi vjetor i energjisë","","kWh/a","2,534","2,534","4,164","3,516","4,456","4,683"]
["Efikasiteti nominal","Annual energy consumption","","kWh","840","","","1,230","1,770"]
["","EER","","","4.05","","","3.86","3.39"]
["","COP","","","4.08","","","3.95","3.42"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","","","A","A"]
["","","Ngrohje","","A","","","A","B"]
["Kapaciteti ngrohës","Nom.","","kW","7.5","","","10.8","13.5"]
["Shënime","","","","(1) - Konsumi vjetor i energjisë është në përputhje me Direktivën e etiketimit të energjisë 2002/31/EC","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - SEER dhe SCOP janë në përputhje me EN 14825","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]