{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.02","0.02","0.03"]
["","Ngrohje","","Nom.","kW","0.02","0.03","0.03"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","600","600","600"]
["","","","Gjerësia","mm","750","750","750"]
["","","","Thellësia","mm","238","238","238"]
["Pesha","Njësia","","","kg","17","17","17"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","8.7","9.2","11.6"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","7","7","9"]
["","","","I ulët","m³/min","4.9","4.9","6.6"]
["","","","Funksionim pa zhurmë","m³/min","4.1","4.1","5.4"]
["","","Ngrohje","I lartë","m³/min","9.2","9.8","12.8"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","7.2","7.2","10"]
["","","Ngrohje","I ulët","m³/min","5.6","5.6","8.4"]
["","","","Funksionim pa zhurmë","m³/min","4.1","4.1","5.9"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","52","53","61"]
["","Ngrohje","","","dBA","52","53","62"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","38","39","44"]
["","","","Mesatar","dBA","32","32","38"]
["","","","I ulët","dBA","25","25","31"]
["","","","Funksionim pa zhurmë","dBA","20","20","27"]
["","Ngrohje","","I lartë","dBA","38","39","46"]
["","","","Mesatar","dBA","32","32","40"]
["","","","I ulët","dBA","25","25","35"]
["","","","Funksionim pa zhurmë","dBA","19","19","29"]
["Agjenti ftohës","GWP","","","","675","675","675"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.4","6.4","6.4"]
["","Gazi","","Dia. jasht.","mm","9.5","9.5","12.7"]
["","Kullimi","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Telekomandë me tela","","","","BRC073A1","BRC073A1","BRC073A1"]
["Aksesore Standarde","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Furnizimi me energji","Emri","","","","V1","V1","V1"]
["","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m"]
["Aksesore Standarde","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]