{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B / RXTM-A"]
[]
[]
[]
[]
["","","","","FVXTM30B2V1B / RXTM30A2V1B"]
["Kapaciteti ftohës","Min.","","kW","1.2"]
["","Nom.","","kW","3"]
["","Maks.","","kW","4.4"]
["Kapaciteti ngrohës","Min.","","kW","1.2"]
["","Nom.","","kW","3.2"]
["","Maks.","","kW","6.2"]
["Efikasiteti nominal","EER","","","4.35"]
["","COP","","","4.45"]
["","Konsumi vjetor i energjisë","","kWh","345"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","3"]
["","SEER","","","7.5"]
["","Konsumi vjetor i energjisë","","kWh/a","140"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","3"]
["","SCOP/A","","","4.75"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","3"]
["","Konsumi vjetor i energjisë","","kWh/a","884"]
["Shënime","","","","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","(2) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","(3) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(4) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]