{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXDQ-M9"]
[]
[]
[]
[]
["","","","","FXDQ20M9V3B9","FXDQ25M9V3B9"]
["Agjenti ftohës","Lloji","","","R-410A","R-410A"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35","6.35"]
["","","Lloji","","Lidhje konike","Lidhje konike"]
["","Gazi","Dia. jasht.","mm","12.7","12.7"]
["","","Lloji","","Lidhje konike","Lidhje konike"]
["","Kullimi","","","I.D. 21.6, O.D. 27.2","I.D. 21.6, O.D. 27.2"]
["Boshllëku i kërkuar i tavanit >","mm","","","250","250"]
["Dimensionet","Njësia","Gjerësia","mm","502","502"]
["","","Thellësia","mm","652","652"]
["","","Lartësia","mm","230","230"]
["Veshja e jashtme","Materiali","","","Çelik i galvanizuar","Çelik i galvanizuar"]
["","Ngjyra","","","Pa bojë","Pa bojë"]
["Pesha","Njësia","","kg","17","17"]
["Power supply","Faza","","","1~","1~"]
["","Frekuenca","","Hz","50","50"]
["","Emri","","","V1","V1"]
["","Tensioni","","V","230","230"]
["Shënime","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]