{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Aksesore Standarde","Deklaratë konformiteti","","","","1"]
["Pesha","Njësia","","","kg","173"]
["Agjenti ftohës","GWP","","","","1.0"]
["","Ngarkesa","","","kg","3.20"]
["Motori i vent.","Fuqia","","","W","350"]
["Shkëmbyesi i nxehtësisë","Lloji","","","","Bobinë me fletë të kryqëzuara"]
["Dimensionet","Njësia","","Gjerësia","mm","635"]
["","","","Thellësia","mm","765"]
["","","","Lartësia","mm","1,680"]
["Veshja e jashtme","Ngjyra","","","","E bardhë fildishi"]
["Ventilatori","Lloji","","","","Ventilatori i helikës"]
["","Niveli i qarkullimit të ajrit","Ftohje","Nom.","m³/min","102"]
["","Sasia","","","","1"]
["Power supply","Faza","","","","3N~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","380-415"]
["Shënime","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Kompresori 1"]
["","","","","","(3) - Kompresori 2"]
["","","","","","(4) - Kompresori 3"]
["","","","","","(5) - Ngarkimi i njësisë në fabrikë"]
["","","","","","(6) - Vetëm K65 me D.P. 120 bar lejohet të përdoret për lidhjet e tubacioneve të ajrit të kondicionuar."]
["","","","","","(7) - Presioni i valvulës së sigurisë tregohet si presioni i matësit."]
["","","","","","(8) - Vetëm K65 me D.P. 90 bar lejohet të përdoret për tubacionet e ftohjes."]