{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Lloji","","","","","Pastrues ajri që krijon lagështi"]
["Përdorimi","","","","","Lloj që qëndron në dysheme"]
["Veshja e jashtme","Ngjyra","","","","E bardhë (N9. 0)"]
["Dimensionet","Njësia","","Lartësia","mm","600 (5)"]
["","","","Gjerësia","mm","395"]
["","","","Thellësia","mm","287"]
["Pesha","Njësia","","","kg","12.5"]
["Sipërfaqja e hapësirës së përdorur","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Funksioni për pastrimin e ajrit","Fuqia në hyrje","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Pa zhurmë","kW","0.008"]
["Funksioni për krijimin e lagështisë","Fuqia në hyrje","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Pa zhurmë","kW","0.011"]
["","Kapaciteti i rezervuarit të ujit","","","l","3.6"]
["Niveli i presionit të zhurmës","Funksioni për pastrimin e ajrit","","Turbo","dBA","54"]
["","","","Mesatar","dBA","37"]
["","","","I ulët","dBA","27"]
["","","","Pa zhurmë","dBA","18"]
["","Funksioni për krijimin e lagështisë","","Turbo","dBA","54"]
["","","","Mesatar","dBA","37"]
["","","","I ulët","dBA","27"]
["","","","Pa zhurmë","dBA","23"]
["Ventilatori","Niveli i qarkullimit të ajrit","Funksioni për pastrimin e ajrit","Turbo","m³/h","420"]
["","","","Mesatar","m³/h","210"]
["","","","I ulët","m³/h","132"]
["","","","Pa zhurmë","m³/h","60"]
["","","Funksioni për krijimin e lagështisë","Turbo","m³/h","420"]
["","","","Mesatar","m³/h","210"]
["","","","I ulët","m³/h","132"]
["","","","Pa zhurmë","m³/h","102"]
["Metoda e grumbullimit të pluhurit","","","","","Filtri elektrostatik HEPA"]
["Metoda e largimit të aromave","","","","","Flash Streamer + katalist aromatizues"]
["Aksesore Standarde","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Kablloja elektrike","m","","","","2"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50/60"]
["","Tensioni","","","V","220-240/220-230"]
["Shënime","","","","","(1) - Sipërfaqja e mbulimit është e përshtatshme për funksionimin e njësisë së shpejtësisë maksimale të  ventilatorit (HH). Sipërfaqja e mbulimit ku përdoret tregon hapësirën ku një sasi e caktuar pluhuri mund të hiqet për 30 minuta."]
["","","","","","(2) - Konvertuar në standardet NRCC nga vlerat e testimit në përputhje me JEM1467."]
["","","","","","(3) - Nivelet e zhurmës gjatë funksionimit janë mesatarja e vlerave të matura në 1 m largësi nga pjesa e përparme, e majtë, e djathtë dhe e sipërme e njësisë. (Kjo është e barabartë me vlerën në një dhomë anekoike)"]