{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A9"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B9","RXA25A5V1B9","RXA35A5V1B9"]
["Dimensionet","Njësia","","Lartësia","mm","550","550","550"]
["","","","Gjerësia","mm","840","840","840"]
["","","","Thellësia","mm","350","350","350"]
["Pesha","Njësia","","","kg","32","32","32"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","46.0","46.0","49.0"]
["","Ngrohje","","Nom.","dBA","47.0","47.0","49.0"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32"]
["","Mbushja","","","kg","0.76","0.76","0.76"]
["","Mbushja","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","20","20","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15.0","15.0","15.0"]
["Aksesore Standarde","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]