{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-A"]
[]
[]
[]
[]
["","","","","","RXF20A2V1B","RXF20A5V1B","RXF25A2V1B","RXF25A5V1B","RXF35A2V1B","RXF35A5V1B","RXF50A2V1B","RXF60A2V1B","RXF71A2V1B","RXF71A5V1B"]
["Dimensionet","Njësia","","Lartësia","mm","550","550","550","550","550","550","735","735","734","734"]
["","","","Gjerësia","mm","658","658","658","658","658","658","825","825","870","870"]
["","","","Thellësia","mm","275","275","275","275","275","275","300","300","373","373"]
["Pesha","Njësia","","","kg","26","26","26","26","28","28","47","47","50.0","50.0"]
["Compressor","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°C DB","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Maks.","°C DB","46","46","46","46","46","46","46","46"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","","","","","","47","49"]
["","","","Nom.","dBA","46","46","46","46","48","48","","","52","52"]
["","Ngrohje","","I lartë","dBA","","","","","","","49","49"]
["","","","Nom.","dBA","47","47","47","47","48","48","","","52","52"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mbushja","","","kg","0.65","0.65","0.65","0.65","0.70","0.70","1.40","1.45","1.15","1.15"]
["","Mbushja","","","tCO2Eq","0.44","0.44","0.44","0.44","0.48","0.48","0.95","0.98","0.78","0.78"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","15","15","15","15","15","15","30","30","30","30"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","12","12","12","12","12","12","20.0","20.0","20","20"]
["Aksesore Standarde","Installation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Kompresori","Lloji","","","","","","","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Aksesore Standarde","Drain cap","","","","","","","","","","","","3","3"]