{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","30.6","30.6"]
["","","Ngrohje","Super e ulët","m³/min","27.2","27.2"]
["","","","Super e ulët","cfm","1080","1080"]
["","","Ngrohje","Super e ulët","cfm","960","960"]
["Dimensionet","Njësia","","Lartësia","mm","550","550"]
["","","","Gjerësia","mm","858","858"]
["","","","Thellësia","mm","330","330"]
["Pesha","Njësia","","","kg","40","40"]
["Compressor","Type","","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°C DB","-10","-10"]
["","","","Maks.","°C DB","46","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-25","-25"]
["","","","Maks.","°CWB","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","48","48"]
["","","","I ulët","dBA","44","44"]
["","Ngrohje","","I lartë","dBA","49","49"]
["","","","I ulët","dBA","45","45"]
["Agjenti ftohës","Lloji","","","","R-410A","R-410A"]
["","Mbushja","","","kg","1","1"]
["","Mbushja","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","20","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - IU","Maks.","m","15","15"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]