{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8"]
["Dimensionet","Njësia","","Lartësia","mm","610"]
["","","","Gjerësia","mm","923"]
["","","","Thellësia","mm","367"]
["Pesha","Njësia","","","kg","40"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","600"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°C DB","-10"]
["","","","Maks.","°C DB","50 (1), 46 (1)"]
["","Ngrohje","Ambienti","Min.","°C WB","-21 (1), -15 (1)"]
["","","","Maks.","°C WB","18"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","48"]
["","Ngrohje","","Nom.","dBA","49"]
["Agjenti ftohës","Lloji","","","","R-32"]
["","Mbushja","","","kg","0.95"]
["","Mbushja","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","30"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","20"]
["Aksesore Standarde","Installation manual","","","","1"]
["","Drain joint","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","LOT10 Energy Label","","","","1"]
["","Drain cap","","","","3"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]
["Shënime","","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","","(3) - Përmban gaze të fluorinuara të efektit serrë"]