{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXQ-A"]
[]
[]
[]
[]
["","","","","","RXQ25AMV1B","RXQ35AMV1B"]
["Dimensionet","Njësia","","Lartësia","mm","550","550"]
["","","","Gjerësia","mm","740","740"]
["","","","Thellësia","mm","337","337"]
["Pesha","Njësia","","","kg","23.0","25.5"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","10","10"]
["","","","Maks.","°CDB","46","46"]
["","Ngrohje","Ambienti","Min.","°C WB","-15","-15"]
["","","","Maks.","°C WB","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","47.0","47.0"]
["Agjenti ftohës","Lloji","","","","R-32","R-32"]
["","Mbushja","","","kg","0.500","0.710"]
["","Mbushja","","","tCO2Eq","0.340","0.480"]
["","GWP","","","","675.0","675.0"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","15","15"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","10.0","10.0"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]