{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","47","","47","","48","48","48"]
["","Ftohje","","I lartë","dBA","46","","46","","48","48","48"]
["Aksesore Standarde","Tapë kullimi","","","","","","","","1","1","1"]
["","Manual instalimi","","","","1","","1","","1","1","1"]
["Agjenti ftohës","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Lloji","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","780","","780","","780","790","670"]
["","","Ngrohje","Super e ulët","rpm","740","","740","","740","780","670"]
["Lidhjet e tubacioneve","Ndryshimi i nivelit","IU - OU","Maks.","m","15","","15","","15","15","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","","0.02 (për gjatësinë e tubave që kalojnë 10m)","","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["Kompresori","Type","","","","Kompresor me lëkundje i izoluar hermetikisht","","Kompresor me lëkundje i izoluar hermetikisht","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","765","","765","","765","765","825"]
["","","","Thellësia","mm","285","","285","","285","285","300"]
["","","","Lartësia","mm","550","","550","","550","550","735"]
["Pesha","Njësia","","","kg","34","","34","","34","39","47"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Super e ulët","cfm","","","","","904","960","1,522"]
["","","Ftohje","Super e ulët","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Faza","","","","1~","","1~","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","","50","","50","50","50"]
["","Tensioni","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit","","(4) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit","","(4) - Përmban gaze të fluorinuara të efektit serrë","(4) - Përmban gaze të fluorinuara të efektit serrë","(4) - Përmban gaze të fluorinuara të efektit serrë"]
["Aksesore Standarde","Bashkues (kullim)","","","","1","","1"]
["Shënime","","","","","(5) - Përmban gaze të fluorinuara të efektit serrë","","(5) - Përmban gaze të fluorinuara të efektit serrë"]
["Dimensionet","Njësia","","Lartësia","mm","","550","","550"]
["","","","Gjerësia","mm","","765","","765"]
["","","","Thellësia","mm","","285","","285"]
["Pesha","Njësia","","","kg","","34","","34"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","","780","","780"]
["","","Ngrohje","Super e ulët","rpm","","740","","740"]
["Kompresori","Type","","","","","Kompresor rrotullues i mbyllur hermetikisht","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","","-10","","-10"]
["","","","Maks.","°CDB","","46","","46"]
["","Ngrohje","Ambienti","Min.","°CWB","","-15","","-15"]
["","","","Maks.","°CWB","","18","","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","46","","46"]
["","Ngrohje","","I lartë","dBA","","47","","47"]
["Agjenti ftohës","Lloji","","","","","R-410A","","R-410A"]
["","Mbushja","","","kg","","1.0","","1.0"]
["","Mbushja","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","","20","","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","0.02 (për gjatësinë e tubave që kalojnë 10m)","","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","","15","","15"]
["Aksesore Standarde","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Furnizimi me energji","Faza","","","","","1~","","1~"]
["","Frekuenca","","","Hz","","50","","50"]
["","Tensioni","","","V","","220-240","","220-240"]