{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","","","48"]
["","Ftohje","","I lartë","dBA","","","48"]
["Aksesore Standarde","Manual instalimi","","","","","","1"]
["","Etiketa e ngarkesës së ftohësit","","","","","","1"]
["","Etiketa në shumë gjuhë për gazet e fluoruara të efektit serë","","","","","","1"]
["","Tapë kullimi (vetëm modelet me pompë nxehtësie)","","","","","","1"]
["Antipiretik","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Ngarkesa","","","kg","","","1.2"]
["","Lloji","","","","","","R-410A"]
["Motori i vent.","Shpejtësia","Ftohje","Super e ulët","rpm","","","780"]
["","","Ngrohje","Super e ulët","rpm","","","740"]
["Diapazoni i funksionimit","Ftohja","Ambienti","Maks.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Ngrohje","Ambienti","Maks.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Lidhjet e tubacioneve","Ndryshimi i nivelit","IU - OU","Maks.","m","","","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["Kompresori","Lloji","","","","","","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","","","765"]
["","","","Thellësia","mm","","","285"]
["","","","Lartësia","mm","","","550"]
["Pesha","Njësia","","","kg","","","34"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Super e ulët","cfm","","","904"]
["","","","Super e ulët","m³/min","","","25.6"]
["","","Ftohje","Super e ulët","m³/min","","","30.1"]
["","","","Super e ulët","cfm","","","1,063"]
["Power supply","Faza","","","","","","1~"]
["","Frekuenca","","","Hz","","","50"]
["","Tensioni","","","V","","","220-240"]
["Shënime","","","","","","","(1) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","30.1","30.1"]
["","","Ngrohje","Super e ulët","m³/min","25.6","25.6"]
["","","","Super e ulët","cfm","1063","1063"]
["","","Ngrohje","Super e ulët","cfm","904","904"]
["Dimensionet","Njësia","","Lartësia","mm","550","550"]
["","","","Gjerësia","mm","765","765"]
["","","","Thellësia","mm","285","285"]
["Pesha","Njësia","","","kg","34","34"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","780","780"]
["","","Ngrohje","Super e ulët","rpm","740","740"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","46","46"]
["","Ngrohje","","I lartë","dBA","47","47"]
["Agjenti ftohës","Lloji","","","","R-410A","R-410A"]
["","Mbushja","","","kg","1.0","1.0"]
["","Mbushja","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","20","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15","15"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Shënime","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Aksesore Standarde","Drain plug (only heat pump models)","","","","","1"]