{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","","","48","48","50","50"]
["","Ftohje","","I lartë","dBA","","","48","48","49","49"]
["Aksesore Standarde","Manual përdorimi","","","","","","1","1","1","1"]
["","Manual instalimi","","","","","","1","1","1","1"]
["Agjenti ftohës","GWP","","","","","","675","675","675","675"]
["","Ngarkesa","","","kg","","","1.34","1.34","1.34","1.34"]
["","Lloji","","","","","","R-32","R-32","R-32","R-32"]
["Diapazoni i funksionimit","Ftohja","Ambienti","Maks.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Ngrohje","Ambienti","Maks.","°CWB","","","18","18","18","18"]
["","","","Min.","°CWB","","","-20","-20","-20","-20"]
["Lidhjet e tubacioneve","Ndryshimi i nivelit","IU - OU","Maks.","m","","","8","8","8","8"]
["Dimensionet","Njësia","","Gjerësia","mm","","","795","795","795","795"]
["","","","Thellësia","mm","","","300","300","300","300"]
["","","","Lartësia","mm","","","693","693","693","693"]
["Kompresori","Lloji","","","","","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht"]
["Pesha","Njësia","","","kg","","","50","50","50","50"]
["Power supply","Faza","","","","","","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","","","50","50","50","50"]
["","Tensioni","","","V","","","220-240","220-240","220-240","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Përmban gaze të fluorinuara të efektit serrë","(4) - Përmban gaze të fluorinuara të efektit serrë","(4) - Përmban gaze të fluorinuara të efektit serrë","(4) - Përmban gaze të fluorinuara të efektit serrë"]
["Dimensionet","Njësia","","Lartësia","mm","693","693"]
["","","","Gjerësia","mm","795","795"]
["","","","Thellësia","mm","300","300"]
["Pesha","Njësia","","","kg","50","50"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","43","43"]
["","Ngrohje","Ambienti","Min.","°CWB","-20","-20"]
["","","","Maks.","°CWB","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","46","46"]
["","Ngrohje","","I lartë","dBA","46","46"]
["Agjenti ftohës","Lloji","","","","R-32","R-32"]
["","Mbushja","","","kg","1.34","1.34"]
["","Mbushja","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","10","10"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","8","8"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]