{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensionet","Njësia","","Lartësia","mm","870","870"]
["","","","Gjerësia","mm","1,100","1,100"]
["","","","Thellësia","mm","460","460"]
["Pesha","Njësia","","","kg","117","117"]
["Kompresori","Lloji","","","","Kompresor spiral i mbyllur hermetikisht","Kompresor spiral i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-20","-20"]
["","","","Maks.","°CDB","46","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-20","-20"]
["","","","Maks.","°CWB","15","15"]
["Sound power level","Ftohje","","","dBA","73","76"]
["","Ngrohje","","","dBA","76 (1)","79 (1)"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","53","57"]
["","Ngrohje","","Nom.","dBA","60","63"]
["Agjenti ftohës","Lloji","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","GWP","","","","675","675"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","22.2","22.2"]
["","Gjatësia e tubacioneve","Maks.","OU - IU","m","100","100"]
["","","Sistemi","Pa ngarkesë","m","30","30"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","Shihni manualin e instalimit","Shihni manualin e instalimit"]
["Aksesore Standarde","Manual instalimi","","","","1","1"]
["","Masat e përgjithshme të sigurisë","","","","1","1"]
["","Fasheta lidhëse për kabllot","","","","2","2"]
["","Etiketë e heqshme për gazet F","","","","1","1"]
["","Tuba për lidhjen","","","","6","6"]
["Power supply","Faza","","","","3~","3~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","380-415","380-415"]
["Rryma - 50Hz","Amperët maksimalë të siguresës (MFA)","","","A","20","20"]
["Shënime","","","","","(1) - Sipas ENER Lot 21","(1) - Sipas ENER Lot 21"]