{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM010A51"]
[]
[]
[]
[]
["","","","","DCM010A51."]
["Connectable unit","","","","Njësi e brendshme, e jashtme, kuti uji, lloje me ajrosje të pikave të menaxhimit të iTM"]
["Hyrja","PC","Softueri","","Microsoft Windows 7, 8, 8.1, 10, Microsoft Server 2012 dhe 2016"]
["Numri maksimal i njësive të brendshme që lidhen","","","","2,500 (2)"]
["Numri maksimal i njësive të jashtme që lidhen","","","","400 (3)"]
["Shënime","","","","(1) - Versionet e pajtueshme të Oracle PMS: Opera v5.0.03.03 e43, v5.0.04.01 e24, v5.0.04.02 e17, v5.0.04.02 e17, v5.0.04.03 e10, v5.0.05.00 dhe version më të ri"]
["","","","","(2) - 5 x 500 njësi të brendshme për çdo kontrollues iTM"]
["","","","","(3) - 5 x 80 sisteme të jashtme për çdo kontrollues iTM"]
["","","","","(4) - Softuer me shkarkim falas, çelësi i licencës në format fizik (letër)"]
["","","","","(5) - Kërkohet 1 licencë DCM010A51 dhe DCM007A51 për çdo kontrollues iTM"]