{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTM-N"]
[]
[]
[]
[]
["","","","","","RXTM30N2V1B","RXTM40N2V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","49","49"]
["","Ftohje","","Nom.","dBA","48","48"]
["Aksesore Standarde","Manual instalimi","","","","1","1"]
["","Etiketa e ngarkesës së ftohësit","","","","1","1"]
["","Etiketa në shumë gjuhë për gazet e fluoruara të efektit serë","","","","1","1"]
["Agjenti ftohës","Charge","","","TCO2Eq","0.7","0.7"]
["","GWP","","","","675","675"]
["","Ngarkesa","","","kg","1.1","1.1"]
["","Type","","","","R-32","R-32"]
["Fan motor","Speed","Ftohje","Super e ulët","rpm","450","360"]
["","","Ngrohje","Super e ulët","rpm","360","360"]
["Lidhjet e tubacioneve","Ndryshimi i nivelit","IU - OU","Maks.","m","15","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["Kompresori","Lloji","","","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","763","763"]
["","","","Thellësia","mm","312","312"]
["","","","Lartësia","mm","551","551"]
["Pesha","Njësia","","","kg","38","38"]
["Power supply","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Shënime","","","","","(1) - Përmban gaze të fluorinuara të efektit serrë","(1) - Përmban gaze të fluorinuara të efektit serrë"]
["","","","","","(2) - Shiko skicën e veçantë për diapazonin e funksionimit","(2) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]