{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLTRH"]
[]
[]
[]
[]
["","","","","WLTRH."]
["Numri maksimal i njësive të brendshme që lidhen","","","","0"]
["Numri maksimal i njësive të jashtme që lidhen @","","","","0"]
["Veshja e jashtme","Ngjyra","","","E bardhë"]
["Mbulesa","Mbulesa e butonave","","","Jo"]
["","Funksionimi LED","Ngjyra","","E gjelbër"]
["Dimensionet","Njësia","Lartësia","mm","75"]
["","","Gjerësia","mm","60.0"]
["","","Thellësia","mm","25.0"]
["","Njësia e ambalazhuar","Lartësia","mm","380"]
["","","Gjerësia","mm","305"]
["","","Thellësia","mm","195"]
["Pesha","Njësia","","kg","0.036"]
["Ambalazhimi","Materiali","","","Karton"]
["","Pesha","","kg","0.0084"]
["Temperatura e ambientit","Funksionimi","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Ruajtja","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Temperatura e ambientit-=-Lagështia relative <-=-%","","%","100"]
["Instalimi","","","","Instalimi i brendshëm"]